## Solution Projects:

1. AnalysisLibrary: Contains codes for designing and calibrating high-rise buildings to NMFS models.
2. ResultsVisualizationUtility: helper to launch the AnalysisLibrary (Empty Project.)
3. GISChapter: Reading Neighbours properties from legacy data (previous), distributing models to Areas inventory, then reading the result from R2D resulting .CSV files.

AnalysisLibrary:

|  |  |
| --- | --- |
| **Class/ Module** | **Function** |
| Project | The start class contains the main run function. |
| ModelState | Enum defines the current stage in the process, |
| LayoutUtility | The properties of the defined layout (location of columns and shear walls) |
| DetailedModel | Class to represent a model for its detailed modeling criteria |
| FloorsGroup | Group of similar floors. |
| ReinforcementUtility | The class contains functions for designing columns and shear walls |
| GridSystem | Class Capture X, Y, and Z axis and generate nodes locations so they are not repeated. |
| ModeShapeData | Class for capturing a solved mode shape |
| PushOverResults | Class for capturing a solved pushover case. |
| IDsManager | The class generates IDs for opensees elements. |
| ModelMaterialsInfo | The class captures the properties of all material in the model |
| LoadCase | Base class for a load case in opensees, the parent for GravityLoadCase, ModalAnalysisLoadCase, PushOverLoadCase |
| ModelEstimationEntity | The class contains functions to calculate a bill of materials after design. |
| OpenSeesTranslator | Class organizes writing tcl files and runs opensees as a background process. |
| BaseCommand | Base Class for all opensees wrapping commands, such as BaseNode, Element, OpenSeesMaterial |
| Element | Base Class for Element commands, the parent for ZeroLengthElement,FrameElasticElement, FrameNonLinearElement |
| OpenSeesMaterial | Base Class for material command in opensees, the parent for  PlateFromPlaneStressMaterial, PlaneStressUserMaterial, ElasticMaterial, HystericMaterial, ParallelMaterial, Concrete02Material, ConcreteUniaxialMaterial, PlateRebarMaterial, SteelUniAxialMaterial |
| Region | Base class for opensees region commands wrapping classes; ElementsRegion, Nodes2DRegion, MasterNodesRegion, BaseNodesRegion |
| Section | Base Class for opensees sections commands; SectiongAggregator, LayeredShell, ElasticShellSection, FiberSection |
| ExcelWriterUtiliy | A class contains functions for writing results in Excel sheets in the bin folder. |
| SimplifiedModel | A class represents a simplified models (NMFS) properties |
| CalibrationUnit | A class contains functions for calibrating a detailed model to NMFS model. |

Main Run Function:

A screenshot of a computer program

Description automatically generated with medium confidence

GISChapter:

|  |  |
| --- | --- |
| **Class/ Module** | **Function** |
| GISProject | The start class contains the main run function. |
| ProjectState | Enum defines the current stage in the process, |
| ArchTypesGroup | A class represents a group of archetypes model as defined in Chapter 5 |
| ArchType | A class represents a model archetype. The properties are Label, YearBuilt, NumberOfStories, Occupancy, StructureType, and PlanArea |
| Neighbour | A class represents a neighbor in the map, the properties are Name, Usage, NoOfbuildings, Polygon (Footprint), and ID |
| BuildingModel | Class represents a model of an archetype existing in a certain neighbour. The properties are ArchType, BuildingResult, and Count (how many it is repeated in the same area) |
| BuildingResult | A Class contains loss estimation parameter |
| DeterminsticParameter | A class contains functions to add/multiply a deterministic parameter |
| PropbabilisticParameter | A class contains functions to add/multiply a probabilistic parameter |

Main Run Function:

A screenshot of a computer program

Description automatically generated with medium confidence